**Meitler Consulting, Inc.**

16979 Chieftain Rd. Tonganoxie, KS 66086

Phone: 913-422-9339

Emergency Phone: 913-422-9339

Fax: 913-845-2950

**MC-MCM**

**30/70 Blend by Volume of Organoclay and 6 x 30 Mesh Anthracite Coal Safety Data Sheet**

Revision Date:01/19/2021

**SECTION 1: Identification of the substance/mixture and of the company/undertaking**

1.1 - Product Identifier

Product Name: MC-MCM

1.2 - Relevant identified uses of the substance or mixture and uses advised against

Use of the substance/mixture: Filtration

1.3 - Details of the supplier of the safety data sheet

Meitler Consulting, Inc

16979 Chieftain Rd.

Tonganoxie, KS 66086

(P) 913-422-9339

(F) 913-845-2950

[www.mciclay.com](http://www.mciclay.com)

1.4 - Emergency telephone number

Emergency number: 1-913-422-9339

**Section 2: Hazards Identification**

2.1 - Classification of the substance or mixture


GHS-US classification

Eye Dam. 1 H318

STOT SE 3 H335

2.2 - Label Elements

GHS-US labelling

Hazard pictograms (GHS-US) 

Signal word (GHS-US): Danger

Hazard statements (GHS-US):

H318 - Causes serious eye damage

H335 - May cause respiratory irritation

Precautionary statements (GHS-US) :

P261 - Avoid breathing dust/fume/gas/mist/vapours/spray

P271 - Use only outdoors or in a well-ventilated area

P280 - Wear protective gloves/protective clothing/eye protection/face protection

P304+P340 - IF INHALED: Remove person to fresh air and keep comfortable for breathing

P305+P351+P338 - If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing

P310 - Immediately call a POISON CENTER/doctor/…

P312 - Call a POISON CENTER/doctor/…/if you feel unwell

P403+P233 - Store in a well-ventilated place, Keep container tightly closed

P405 - Store locked up

P501 - Dispose of contents/container to…..

2.3 - Other Hazards

No additional information available

2.4 - Unknown acute toxicity (GHS US) No data available

**SECTION 3: Composition/information on ingredients**

3.1 - Substances

Not applicable

3.2 - Mixture

|  |  |  |  |
| --- | --- | --- | --- |
| **Name Product Identifier % GHS-US Classification** | | | |
| Zeolite (CAS No.) 1318-02-1 62 - 64 STOT SE 3, H335 | | | |
| Coal, anthracite (CAS No.) 8029-10-5 25.98 - 27.98 | | | |
| Water (CAS No.) 7732-18-5 3.56 - 9.46 Not classified | | | |
| N,N,N-Trimethyl-1-hexadecanaminium chloride | (CAS No.) 112-02-7 | 2.46 - 4.46 | Skin Irrit. 2, H315  Eye Dam. 1, H318  Aquatic Acute 1, H400 |

**SECTION 4: First aid measures**

4.1 - Description of first aid measures

First-aid measures after inhalation: Remove person to fresh air. If not breathing, administer CPR or artificial respiration. Get immediate medical attention.

First-aid measures after skin contact: If skin reddening or irritation develops, seek medical attention.

First-aid measures after eye contact: Immediately flush eyes with plenty of water for at least 15 minutes. If irritation

Persists, get medical attention.

First-aid measures after ingestion: If the material is swallowed, get immediate medical attention or advice. DO

NOT induce vomiting unless directed to do so by medical personnel.

4.2 - Most important symptoms and effects, both acute and delayed

Symptoms/injuries after inhalation: May cause respiratory irritation. Symptoms/injuries after skin contact: May cause skin irritation. Symptoms/injuries after eye contact: Causes serious eye irritation. Symptoms/injuries after ingestion: May be harmful if swallowed.

4.3 - Indication of any immediate medical attention and special treatment needed

No additional information available

**SECTION 5: Firefighting measures**

5.1 - Extinguishing media

Suitable extinguishing media: If involved with fire, flood with plenty of water. Unsuitable extinguishing media: None.

5.2 - Special hazards arising from the substance or mixture

Fire hazard: None known. Explosion hazard: None known.

5.3 - Advice for firefighters

Protection during firefighting: Firefighters should wear full protective gear.

**SECTION 6: Accidental release measures**

6.1 - Personal precautions, protective equipment and emergency procedures

General measures: Avoid contact with the skin and the eyes.

For non-emergency personnel: No additional information available

For emergency responders: No additional information available

6.2 - Environmental precautions

None

6.3 - Methods and material for containment and cleaning up

For containment: If possible, stop flow of product.

Methods for cleaning up: Shovel or sweep up and put in a closed container for disposal.

6.4 - Reference to other sections

No additional information available

**SECTION 7: Handling and storage**

7.1 - Precautions for safe handling

Precautions for safe handling: Avoid contact with eyes.

7.2 - Conditions for safe storage, including any incompatibilities

Storage conditions: Protect containers from physical damage. Store in a dry, cool, well-ventilated area.

7.3 - Specific end use(s)

No additional information available

**SECTION 8: Exposure controls/personal protection**

8.1 - Control parameters

**Coal, anthracite (8029-10-5)**

USA ACGIH ACGIH TWA (mg/m³) 0.4 mg/m³

8.2 - Exposure controls

Appropriate engineering controls: Local exhaust and general ventilation must be adequate to meet exposure standards.

Hand protection: Use impervious gloves. Eye protection: Safety glasses.

Skin and body protection: Wear suitable working clothes.

Respiratory protection: If airborne concentrations are above the applicable exposure limits, use NIOSH

approved respiratory protection.

**SECTION 9: Physical and chemical properties**

9.1 - Information on basic physical and chemical properties

Physical state: Solid Appearance: Irregular shaped Colour: White/black

Odour: No data available

Odour threshold: No data available

pH: No data available

Relative evaporation rate (butylacetate=1): No data available

Melting point: No data available

Freezing point: No data available

Boiling point: No data available

Flash point: No data available

Self ignition temperature: No data available

Decomposition temperature: No data available

Flammability (solid, gas): No data available

Vapour pressure: No data available

Relative vapour density at 20 °C: No data available

Relative density: 54-56 lb/ft3

Solubility: No data available

Log Pow : No data available

Log Kow : No data available

Viscosity, kinematic: No data available

Viscosity, dynamic: No data available

Explosive properties: No data available

Oxidising properties: No data available

Explosive limits: No data available

9.1 - Other information

No additional information available

**SECTION 10: Stability and reactivity**

10.1 - Reactivity

No additional information available

10.2 - Chemical stability

Stable under normal conditions.

10.3 - Possibility of hazardous reactions

Will not occur

10.4 - Conditions to avoid

None

10.5 - Incompatible materials

Strong oxidizing and reducing agents such as ozone, liquid oxygen, or chlorine.

10.6 - Hazardous decomposition products

Carbon monoxide may be generated in the event of a fire. Organic chlorides, amines, hydrogen chloride may be produced.

**SECTION 11: Toxicological information**

11.1 - Information on toxicological effects

Acute toxicity: Not classified

|  |
| --- |
| **Zeolite (1318-02-1)** |
| LD50 oral rat 5000 mg/kg |
| LD50 dermal rabbit > 2000 mg/kg |
| LC50 inhalation rat (mg/l) 2.4 mg/l (Exposure time: 1 h) |
| ATE (oral) 5000 mg/kg |

**N,N,N-Trimethyl-1-hexadecanaminium chloride (112-02-7)**

LD50 dermal rabbit 4300 uL/kg/24H;

Skin corrosion/irritation: Not classified

Serious eye damage/irritation: Causes serious eye damage.

Respiratory or skin sensitisation: Not classified

Germ cell mutagenicity: Not classified

Carcinogenicity: Not classified

**Zeolite (1318-02-1)**

IARC group 3

Reproductive toxicity: Not classified

Specific target organ toxicity (single exposure): May cause respiratory irritation.

Specific target organ toxicity (repeated exposure): Not classified

Aspiration hazard: Not classified

**SECTION 12: Ecological information**

12.1 - Toxicity

|  |  |
| --- | --- |
| **Zeolite (1318-02-1)** | |
| LC50 fishes 1 | 1800 mg/l (Exposure time: 96 h - Species: Brachydanio rerio [semi-static]) |
| EC50 Daphnia 1 | 1000 - 1800 mg/l (Exposure time: 48 h - Species: Daphnia magna) |
| EC50 other aquatic organisms 1 | 18 mg/l (Exposure time: 96 h - Species: Desmodesmus subspicatus) |
| LC50 fish 2 | 3200 - 5600 mg/l (Exposure time: 96 h - Species: Oryzias latipes [semi-static]) |

12.2 - Persistence and degradability

No additional information available

12.3 - Bioaccumulative potential

No additional information available

12.4 - Mobility in soil

No additional information available

12.5 - Other adverse effects

No additional information available

**SECTION 13: Disposal considerations**

13.1 - Waste treatment methods

Waste disposal recommendations: Dispose of contents/container in accordance with local/regional/national/international regulations.

**SECTION 14: Transport information**

In accordance with DOT / ADR / RID / ADNR / IMDG / ICAO / IATA

14.1 - UN number

Not applicable

14.2 - UN proper shipping name

Not applicable

**SECTION 15: Regulatory information**

15.1 - US Federal regulations

**N,N,N-Trimethyl-1-hexadecanaminium chloride (112-02-7)**

Listed on the United States TSCA (Toxic Substances Control Act) inventory

15.2 - US State regulations

No additional information available

**SECTION 16: Other information**

Full text of H-phrases:

|  |  |
| --- | --- |
| Aquatic Acute 1 | Hazardous to the aquatic environment - Acute Hazard  Category 1 |
| Eye Dam. 1 Serious eye damage/eye irritation Category 1 | |
| Skin Irrit. 2 skin corrosion/irritation Category 2 | |
| STOT SE 3 | Specific target organ toxicity (single exposure) Category 3 |
| H315 Causes skin irritation | |
| H318 Causes serious eye damage | |
| H335 May cause respiratory irritation | |
| H400 Very toxic to aquatic life | |

NFPA health hazard : 2 - Intense or continued exposure could cause temporary incapacitation or possible residual injury unless prompt

medical attention is given.

NFPA fire hazard : 0 - Materials that will not burn.

NFPA reactivity : 0 - Normally stable, even under fire exposure conditions, and are not reactive with water

*Copyright 2017 Meitler Consulting, Inc. License granted to make unlimited paper copies for internal use only. The above information is believed to be correct but does not purport to be all inclusive and shall be used only as a guide. This information is based on our current knowledge and is intended to describe the product for the purposes of health, safety and environmental requirements only. It should not therefore be construed as guaranteeing any specific property of the product. Meitler Consulting, Inc. makes no warranty, either expressed or implied, including any warranties of merchantability and fitness for a particular purpose.*