Safety Data Sheet

MC-1870

Revision: January 15, 2021

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Section 1: | | IDENTIFICATION | | | |
| 1.1 Product Name: MC-1870  1.2 Other Identification: | |  |  |
| Chemical Family: | | Inorganic salt solution. |  |
| Formula: | | casx |  |
| 1.3 Recommended Use of Chemical: | | Metal precipitant |  |
| 1.4 Manufacturer: | | Meitler Consulting, Inc.  16979 Chieftain Rd.  Tonganoxie, Kansas 66086 |  |
| Information: | | (913) 422-9339 |  |
| 1.5 Emergency Contact: | | Meitler Consultings, Inc. | (913) 422-9339 |
|  | | CHEMTREC | (800) 424-9300 |

|  |  |  |  |
| --- | --- | --- | --- |
| Section 2: | HAZARD(S) IDENTIFICATION | | |
| 2.1 Hazard Classification: | | Health Acute Toxicity-Oral | Category 4 | |
|  | | Acute Toxicity-Dermal | Category 4 | |
|  | | Acute Toxicity-Inhalation | Category 4 | |
|  | | Skin Corrosion/lrritation | Category 2 | |
|  | | Eye Damage/lrritation | Category 2A | |
|  | | Physical Corrosive to metals | Category 1 | |
| 2.2 Signal Word: | | Warning |  | |
| 2.3 Hazard Statement(s): | | Harmful if swallowed.  Harmful in contact with skin.  Harmful if inhaled.  Causes skin irritation.  Causes serious eye irritation.  May be corrosive to metals. |  | |

2.4 Symbol(s):

  

2.5 Precautionary Statement(s):

2.6 Unclassified Hazard(s):

2.7 Unknown Toxicity Ingredient:

**If swallowed**: Rinse mouth. Call a poison center/doctor/regional medical center if you feel unwell.

**If on skin**: Wash with plenty of water. Take off contaminated clothing and wash before reuse. If skin irritation occurs: Get medical advice. Call a poison center/doctor/regional medical center if you feel unwell.

**If inhaled**: Remove person to fresh air and make comfortable for breathing. Call poison center/doctor/regional medical center if you feel unwell.

**If in eyes**: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. If eye irritation persists: Get medical advice/attention.

Wash hands and face thoroughly with water after handling. Do not eat, drink or smoke when using this product.

Wear neoprene rubber chemical suit, gloves, goggles/full-face shield when handling product.

Avoid breathing product fume/gas/mist/vapors/spray.

Use only outdoors or in well-ventilated area.

Absorb spillage to prevent material damage.

Keep/store in original corrosive resistant container

Dispose of contents/container to chemical waste facility in accordance with local/regional/federal regulations.

Do not allow release to aquatic waterways.

Aquatic toxicity

None

|  |  |
| --- | --- |
| **Section 3:** | **COMPOSITION/INFORMATION on INGREDIENTS** |

3.1 **Chemical Ingredients**: (See Section 8 for exposure guidelines)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Chemical** | **Synonym Common Name** | **CAS No.** | **EINECS No.** |  |
| Calcium polysulfide, CaSx | Lime sulfur, calcium sulfide | 1344-81-6 | 215-709-2 | 24 - 29 |
| Water | Water | 7732-18-5 | 231-791-2 | Remainin % |

|  |
| --- |
| **Section 4: FIRST AID MEASURES** |

**4.1 Symptoms/Effects:**

Acute: Eye contact may cause eye irritation. Repeated or prolonged skin contact may cause skin irritation. Ingestion may irritate the gastrointestinal tract.

Chronic: No known chronic effects.

**4.2 Eyes:** Immediately flush with large quantities of water for 15 minutes. Hold eyelids apart during irrigation to ensure thorough flushing of the entire area of the eye and lids. Obtain medical attention if irritation occurs.

**4.3 Skin:** Immediately flush with large quantities of water. Remove contaminated clothing under a safety shower. Continue rinsing. Obtain medical attention if irritation occurs.

**4.4 Ingestion:** If victim is conscious, give 2 to 4 glasses of water and induce vomiting by touching finger to back of throat. Obtain immediate medical attention.

**4.5 Inhalation:** Remove victim from contaminated atmosphere. If breathing is labored, administer Oxygen. If breathing has ceased, clear airway and start CPR. Obtain immediate medical attention.

|  |  |
| --- | --- |
| **Section 5:** | **FIRE FIGHTING MEASURES** |

**5.1 Flammable Properties:**  (See Section 9, for additional flammable properties)

**NFPA:** Health - 2 Flammability - 0 Reactivity - 1

**5.2 Extinguishing Media:**

**5.2.1 Suitable Extinguishing Media**: Not flammable, use media suitable for combustibles involved in fire.

**5.2.2 Unsuitable Extinguishing Media:** Not applicable.

**5.3 Protection of Firefighters:**

**5.3.1 Specific Hazards Arising from the Chemical:**

|  |  |
| --- | --- |
| **Physical Hazards:**  **Chemical Hazards:** | Heating (flames) of closed or sealed containers may cause violent rupture of container due to thermal expansion of compressed gases.  Heating causes release of Hydrogen sulfide vapors. Vapors are irritating to eyes, |

skin and respiratory tract.

**5.3.2 Protective Equipment and Precautions for Firefighters:**

Heating this product may evolve hydrogen sulfide vapors.

Firefighters should wear self-contained breathing apparatus (SCBA) and full firefighting turnout gear. Keep containers/storage vessels in fire area cooled with water spray.

|  |  |
| --- | --- |
| **Section 6:** | **ACCIDENTAL RELEASE MEASURES** |

**6.1 Personal Precautions:** Use personal protective equipment specified in Section 8. Isolate the release area and deny entry to unnecessary, unprotected and untrained personnel.

**6.2 Environmental Precautions:**

Keep out of "waters of the United States" because of aquatic toxicity (See Section 12).

**6.3 Methods of Containment:**

|  |  |
| --- | --- |
| **Small Release:**  **Large Release:** | Confine and absorb small releases on sand, earth or other inert absorbents.  Shut off release if safe to do so. Dike spill area with earth, sand or other inert absorbents to prevent runoff into surface waterways, storm drains or sewers (aquatic toxicity). |

**6.4 Method for Cleanup:**

|  |  |
| --- | --- |
| **Small Release:**  **Large Release:** | For small areas shovel up absorbed material and place in drums for disposal as a chemical waste.  Recover as much of the spilled product using portable pump and hoses. Use as originally intended or dispose of as a chemical waste. Treat remaining material as |

a small release (above).

|  |  |
| --- | --- |
| **Section 7:** | **HANDLING and STORAGE** |

**7.1 Handling:** Avoid contact with eyes. Use only in a well-ventilated area. Wash thoroughly after handling. Avoid prolonged or repeated breathing of vapors. Avoid prolonged or repeated contact with the skin.

**7.2 Storage:** Store in well-ventilated areas. Do not store combustibles in the area of storage vessels. Keep away from any sources of heat or flame. Store totes and smaller containers out of direct sunlight at moderate temperatures.

|  |
| --- |
| **Section 8: EXPOSURE CONTROLS/PERSONAL PROTECTION** |

**8.1 Exposure Guidelines:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Chemical** | **OSHA PELs** | | **ACGIH TLVs** | |
|  | **TWA** | **STEL** | **TWA** | **STEL** |
| Hydrogen sulfide | None | 20 ppm (Ceiling) | 1 ppm | 5 ppm |
| Calcium polysulfide, CaSx | None | None | None | None |
| Water | None | None | None | None |

**8.2 Engineering Controls:** Use adequate exhaust ventilation to prevent inhalation of product vapors. Keep eye wash/safety shower in areas where product is commonly handled.

**8.3 Personal Protective Equipment (PPE):**

|  |  |
| --- | --- |
| **8.3.1 Eye/Face Protection**:  **8.3.2 Skin Protection:** | Chemical goggles and a full face shield.  Neoprene rubber gloves and suit should be worn to prevent repeated or prolonged contact with the liquid. Wash contaminated clothing prior to |

reuse.

**8.3.3 Respiratory Protection:**

Have self-contained breathing apparatus (SCBA), positive pressure, MSHA/NIOSH (approved or equivalent) available in case of spillage or equipment failure.

**8.3.4 Hygiene Considerations:**

Common good industrial hygiene practices should be followed, such as washing thoroughly after handling and before eating or drinking.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Section 9:** | | **PHYSICAL and CHEMICAL PROPERTIES** | | | | | | |
| 9.1 Appearance: | | | | Ruby-red liquid. |
| 9.2 Odor: | | | | Possible odor of rotten eggs. |
| 9.3 Odor Threshold: | | | | 4.7 ppb (hydrogen sulfide)  11.5 - 11 .7, Typical |
| 9.5 Melting Point/Freezing Point: | | | | 18 to 25 0 F (-7.7 to -3.9 0 C), (Typical) |
| 9.6 Boiling Point: | | | | Not determined |
| 9.7 Flash Point: | | | | Not applicable |
| 9.8 Evaporation Rate: | | | | Not determined |
| 9.9 Flammability: | | | | Not applicable |
| 9.10 Upper/Lower Flammability Limits: | | | | Not applicable |
| 9.11 Vapor Pressure: | | | | Not determined |
| 9.12 Vapor Density: | | | | Not determined |
| 9.13 Relative Density: | | | | 1.27 (10.6 lbs/gal), (Typical) |
| 9.14 Solubility: | | | | Miscible |
| 9.15 Partition Coefficient: | | | | No data available. |
| 9.16 Auto-ignition Temperature: | | | | Not applicable |
| 9.17 Decomposition Temperature: | | | | Not determined |
| 9.18 Viscosity: | | | | 2.95 cSt @ 20 0 C, 2.5 cSt @ 300 c. |
|  | | | | |  | | |
| **Section 10: STABILITY and REACTIVITY** | | | | |  | | |
|  | | | | |  | | |
| 10.1 Reactivity:  10.2 Chemical Stability: | | | | | Strong oxidizers and acids  This is a stable product under normal (ambient) temperature and pressure. | | |
| 10.3 Possibility of Hazardous Reactions: | | | | | Interaction with strong oxidizers, acids or acidic materials. | | |
| 10.4 Conditions to Avoid: | | | | | High heat and fire conditions. Interaction with strong oxidizers or acidic materials (evolution of Hydrogen sulfide vapors). | | |
| 10.5 Incompatible Materials: | | | | | Strong oxidizers can cause explosive mixtures if heated to dryness. Acids, acidic materials and dilution with water will cause the release of highly toxic Hydrogen sulfide vapors. This product is not compatible with Copper, Aluminum or their alloys (i.e. brass, bronze, etc.). These materials of construction should not be utilized in handling systems or storage containers for this product should not be used | | |
| 10.6 Hazardous Decomposition Products: | | | | | Hydrogen sulfide and Oxides of Sulfur. | | |
| **Section 11:** | | | | | **TOXICOLOGICAL INFORMATION** | | | | |

**11.1 Oral:** Oral Rat LD50: 820 mg/kg. (calcium polysulfide)

|  |  |  |  |
| --- | --- | --- | --- |
| **11.2 Dermal:** | | | Dermal Rabbit LD50: > 2,000 mg/kg. (calcium polysulfide) |
| **11.3 Inhalation:** | | | INH-Rat LC50: 3.6mg/L(4 hr. exposure). (calcium polysulfide)  Primary Eye Irritation — Irreversible damage due to high pH. |
| **11.5 Chronic/Carcinogenicity:** | | | Not listed in NTP, IARC or by OSHA. |
| **11.6 Teratology:** | | | No data available. |
| **11.7 Reproduction:** | | | No data available. |
| **11.8 Mutagenicity:** | | | No data available. |
| **Section 12:** | | **ECOLOGICAL INFORMATION** | | | | |
| **2.1 Ecotoxicity:** | | | Green Algae, EC50: 16.4 mg/l. (calcium polysulfide)  Water Flea, EC50: 13.7 mg/l. (calcium polysulfide)  Bluegill, LC50: 52.9 mg/l. (calcium polysulfide)  Fathead Minnow, LC50: 42.9 mg/l. (calcium polysulfide) Rainbow Trout, LC50. 8.8 mg/l. (calcium polysulfide)  Honey Bee LD50: >25 ug ai/Bee. (calcium polysulfide)  Avian LD50: 560 ai/kg. (calcium polysulfide)  Bobwhite Quail LD50: 560 ai/kg body wt. (calcium polysulfide) | | |
| **12.2 Persistence & Degradability:** | | | "Calcium polysulfide present in moist soils and/or on moist foliage is expected to dissociate rapidly; therefore, run-off and erosion into surface waters, as present calcium polysulfide, should be negligible." (EPA, RED) | | |
| **12.3 Bioaccumulative Potential:** | | | This product is not bioaccumulative. | | |
| **12.4 Mobility in Soil:** | | | No data available. | | |
| **12.5 Other Adverse Effects:** | | | None | | |
| **Section 13:** | | **DISPOSAL CONSIDERATIONS** | | | | |

Consult federal, state and local regulations for disposal regulations.

|  |
| --- |
| **Section 14: TRANSPORT INFORMATION** |

**14.1 Basic Shipping Description:**

**14.1.1 Proper Shipping Name:** Calcium polysulfide solution (Not regulated by DOT)

**14.1.2 Hazard Classes:** Not applicable

**14.1.3 Identification Number:** Not applicable

**14.1.4 Packing Group:** Not applicable

**14.1.5 Hazardous Substance:** No

**14.1.6 Marine Pollutant:** No

**14.2 Additional Information:**

**14.2.1 Other DOT Requirements:**

**14.2.1.1 Reportable Quantity:** No

**14.2.1.2 Placard(s):** Not applicable

**14.2.1.3 Label(s):** Not applicable

**14.2.2 USCG Classification:** Not determined.

**14.2.3 International Transportation:**

**14.2.3.1 IMO:** UN3082, Environmentally Hazardous Substance, liquid, n.o.s., 9, PG III (Marine Pollutant – calcium polysulphide)

**14.2.3.2 IATA:** Not regulated

**14.2.3.3 TDG (Canada):** Not regulated

**14.2.3.4 ADR (Europe):** UN3082, Environmentally Hazardous Substance, liquid, n.o.s., 9, PG III (Marine Pollutant – calcium polysulphide)

**14.2.3.5 ADG (Australia):** UN3082, Environmentally Hazardous Substance, liquid, n.o.s., 9, PG III (Marine Pollutant – calcium polysulphide)

**14.2.4 Emergency Response Guide:** Not applicable

**14.2.5 ERAP – Canada:** Not applicable

**14.2.6 Special Precautions:** Not applicable

|  |
| --- |
| **Section 15: Regulatory Information** |

**15.1 U.S. Federal Regulations:**

**15.1.1 OSHA:** This product is considered a hazardous chemical under the Federal OSHA Hazard Communication Standard (29 CFR 1910.1200).

**15.1.2 TSCA:** Product is contained in USEPA Toxic Substance Control Act Inventory.

**15.1.3 CERCLA:** Reportable Quantity – No

**15.1.4 SARA Title III:**

**15.1.4.1 Extremely Hazardous Substance (EHS):** No

**15.1.4.2 Section 312 (Tier II) Ratings:** Immediate (Acute) Yes

Fire No

Sudden Release No

Reactivity No

Delayed (chronic) No

**15.1.4.3 Section 313 (FORM R):**  Not applicable

**15.1.5 RCRA:**  Not applicable

**15.1.6 CAA (Hazardous Air Pollutant/HAP):**  Not applicable

**15.2 International Regulations**:

**15.2.1 Canada:**

**15.2.1.1 WHMIS:** Not determined

**15.2.1.2 DSL/NDSL:**  Listed in NDSL, Record No. 28636

**15.3 State Regulations:**

**CA Proposition 65:** Not applicable

|  |
| --- |
| **Section 16: OTHER INFORMATION** |

*The information above is believed to be accurate and represents the best information currently available to Meitler Consulting Inc. No warranty of merchantability, fitness for any particular purpose, or any other warranty is expressed or is to be implied regarding the accuracy or completeness of this information, the results to be obtained from the use of this information or the product, the safety of this product, or the hazards related to its use. Users should make their own investigations to determine the suitability of the information for their particular purpose and on the condition that they assume the risk of their use thereof. Meitler Consulting, Inc. reserves the right to revise this Safety Data Sheet periodically as new information becomes available.*

**14.1 Basic Shipping Description:**

**14.1.1 Proper Shipping Name:** Calcium polysulfide solution (Not regulated by DOT)

**14.1.2 Hazard Classes:** Not applicable **14.1.3 Identification Number:** Not applicable

**14.1.4 Packing Group:** Not applicable **14.1.5 Hazardous Substance:** No  **14.1.6 Marine Pollutant:** No

**14.2 Additional Information:**

**14.2.1 Other DOT Requirements**